Spar of BAW only, measured on Amber2 lab1 pcb.
port 1 is RF4 side.

Used 97mm long thin coax, with 0.5mm inner-conductor-ends.
Deembedded with 553ps (486degrees one-way), 0.6dB at 2.4GHz.
The inner-conductor-ends correspond to 0.22nH, that has to be subtracted in the simulation (not de-embedded in the s-par).