! Optimal fundamental load for minimum 2nd harmonics.
! In order to get two dots, do the transition between adjacent sweeppoints, otherwise it will interpolate
! and only use two S values, otherwise it will also xtrapolate.
! Minimum of Freq points is 3, otherwise you get an error.
! Date and time: Wed Jun 24 11:31:40 2020
# GHz S MA R 50
2.44	0.35		145
4.8		0.2		120
4.88	0.2		120