! Optimal fundamental load for minimum 2nd harmonics.
! In order to get two dots, do the transition between adjacent sweeppoints, otherwise it will interpolate
! and only use two values, otherwise it will also xtrapolate.
! Date and time: Wed Jun 24 11:31:40 2020
# GHz S MA R 50
2.41		0.2		150
2.44	0.2		150
4.8799	0.2		150
4.88	0.7		150
7.5		0.7		150