! Optimal fundamental load for minimum 2nd harmonics.
! In order to get two dots, do the transition between adjacent sweeppoints, otherwise it will interpolate
! and only use two values, otherwise it will also xtrapolate.
! Date and time: Wed Jun 24 11:31:40 2020
# GHz S MA R 50
2.4	0.5	330
5	0.99	330
