! Optimal fundamental load for minimum 2nd harmonics.
! In order to get two dots, do the transition between adjacent sweeppoints, otherwise it will interpolate
! and only use two values, otherwise it will also xtrapolate.
! Date and time: Wed Jun 24 11:31:40 2020
# GHz S MA R 50
0.01	0.5		150
2.442	0.5		150
2.44201	0.5		210
4.87999	0.5		210
4.88	0.01	120
7.5		0.01	120